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	Project Details

	Project title: 
	Project cost code: 

	Estimated start/end date: 
	Approximate labour cost: 

	Contractors required: ☐ Y ☐ N
	Principal Contractor: 
	☐  Internal (NTPC)     ☐  External (Contractor)

	[bookmark: _GoBack]Detailed project description: 

	High Risk Activities (include checked items in Hazard Assessment section) 

	☐  Civil/site preparation
☐  Confined spaces
☐  Diving operations
☐  Excavation
	☐  Exposure to asbestos
☐  High voltage work
☐  Ice road construction
☐  Line clearing
	☐  Line construction
☐  Rigging & lifting
☐  Scaffolding & shoring
☐  Work around water
	☐  Work at heights > 3m
☐  Other:  
☐  Other: 
☐  Other: 

	Work to be Completed by Contractors

	1
	

	2
	

	3
	

	4
	

	Developed by (Project Manager): 

	Date: 


	Reviewed by (H&S Department): 

Date: 

The following Project Safety Plan is required:
     PSP for Major works ☐  PSP for Minor works ☐
Additional Requirements wording needed: ☐ Y ☐ N 
	Additional Requirements (for procurement docs): 

	Approved by (Manager/Director): 

	Date: 
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Hard copies of this document are considered uncontrolled.  Please refer to the PowerLine for the latest version.
	Hazard Assessment & Control

	Job Steps
	Tools & Equipment
	Major Hazards
	Required Controls 
(reference *SWPs, SJPs, JSAs)

	Step 1 Example:
· Travel to site 
	Example: 
· ATV
	Example: 
· Rugged terrain (crashes)
· Eye damage hazard from branches
· Cuts, scrapes, etc. from branches
	Example: 
· ATV SWP
· Helmet to protect from branches and crashes
· Safety boots, long sleeves, gloves

	Step 2 Example: 
· Cut brush
	Example: 
· Chainsaw
	Example:
· Cuts from saw
· Getting hit by falling trees
	Example:
· Chainsaw Operation SWP
· Tree Felling and Branch Removal SWP
· Chainsaw PPE (safety glasses, hard hat, ballistic pants & boots, gloves)

	Step 3 Example: 
· Pile brush by hand
	Example
· None
	Example: 
· Cuts, scrapes, etc. from branches
· Eye damage hazard from branches
· Muscle strain from lifting
	Example: 
· Gloves, long sleeves, safety boots
· Safety glasses
· Manual handling SWP

	Step 4 Example: 
· Return from site
	Example: 
· ATV
	Example: 
· Rugged terrain (crashes)
· Eye damage hazard from branches
· Cuts, scrapes, etc. from branches
	Example: 
· ATV SWP
· Helmet to protect from branches and crashes
· Safety boots, long sleeves, gloves


* Safe Work Practice (SWP), Safe Job Procedure (SJP), Job Safety Analysis (JSA)
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